Gasflow Sensor (GFS)

The Urban Concept Hydrogen Fuel Cell teams equipped with the Telemetry system shall be required to fit a Vögtlin Red-Y series Hydrogen Flowmeter. This meter shall be fitted according to the Chapter 1 rules and the instructions supplied by the manufacturer.