Do not come to Tech Inspection until you have

a printed technical documentation of your vehicle

OBC Pod and Backbone installed

charged and installed the OBC Battery

charged the vehicle’s main Battery

charged the Joulemeter (The JM for the Supercap in Urban concept H2 doesn't require Charging)

installed the energy sensor(s) (JM, GFM, LFM)

connected the Shutdown Relay

verified the Telemetry System (OBC Pod LED)

Filled-out Self-Inspection Checklist